

Updating the Arduino to Bittern V2-1 build

Unzip the Bittern V2-1 folder and copy to the desktop – it should contain two files and the Xloader folder.



Open the Xloader folder and double click XLoader.exe to launch the application



The small XLoader window should now appear. Click on the three dots … in the blue box upper right and navigate to Data\_log\_bit\_2-1.ino.mega.hex – select this file

Using the drop down window select Mega(ATMEGA2560) as the device and choose the COM port to which the Arduino is connected.

Leave the Baud rate at 115200

Click on upload – the upload only takes a few seconds and when it is complete the LCD display on the gas flow meter should show that it is running Bittern V2-1.

